Machine generated alternative text:
Device Repository 
Version 
vol.oo.oo 
VI.o.16 
4.3.1.0 
41.0.0 
4.3.1.0 
SW-SWV 1,7.14, HW-HVV 1 
SW-SW VI. 7,27, HW-HVV 1 
sw-vol.oo, HW 
sw 
vol.01, HW 
sw 
V3.x, HW-2 
sw 
VI.oo,HW-V1.oo 
Description 
10-Link device based on an IODD file 
10 -Link device based on an IODD file 
PROFINETIO controller CIFX for Firmvvare Version V3.x.x.x. 
Profinet 10 Gateway for Ethercat 
PROFINEr10 controller 
PROFINET 10 Block module in IP67 
PROFINET 10 Block module ln IP67 
Promag 300 500 PROFINErV1.o 
Promag 300 500 PROFINErV1.1 
CODEsys PLC running as PROFINET Device (CIFX based) 
PROFINEr 1/0 device -EtherCAT slave terminal, V2. O 
Edit Locations 
Install... 
Uninstall 
DEteiIs... 
Close 
Location 
System Reçu)sitory 
(c:1ProgramData1CODEsys1Devices) 
Vend or KAII vendors:» 
Vendor 
Endr ess +Hauser 
Turck 
3S - Smart Software Solutions GmbH 
3S - Smart Software Solutions GmbH 
3S - Smart Software Solutions GmbH 
Installed Device Descriptions 
String for text search 
XRN CANbus 
CiR CANopen 
EtherCAT 
Ethernet Adapter 
EtherNe t,'TP 
Home&BuiIding Automation 
e 10-Link Devices 
O IODD 1.1 
Liquphant FTL3x 
I' PT1.6A-XXXX-10L+1141 
e SIO 
J 1939 
Modbus 
PROFINEr 10 
Ethernet Adapter 
PROFINEr 10 Device 
PROFINEr 10 Master 
CIFX PN-contr011er 
EL6631 Profnet Gateway 
PN-ControIIer 
PROFINEr 10 slave 
1/0 
supports RT-c1ass 3 (IRT). 
CODEsys PLC 
Tur ck 
TBEN-S24A1 
TBEN-S2410L 
Promag 300 500 
Promag 300 500 VI.o 
Promag 300 500 VI. 1 
CIFX PROFINET Device 
EL6631-0010 V2.o 
S sercos 
HMI devices 
Turck 
Turck 
Endr ess +Hauser 
Endr ess +Hauser 
3S - Smart Software Solutions GmbHMachine generated alternative text:
PersistentVars 
Etherne t (Etherne t) 
PN Controller (PN-ControIIer) 
jbp21 CrBEN-S2-410L) 
jbp21_I (Basic) 
10 Link Port 2 (PT5V-xxxx-10L+1141(D1)) 
10 Link Port 3 (PT250R-xxxx-10L+1141) 
10 
Diagno 
10 Lin 
Device 
jbp23 
lbp23 
10 
10 
10 
Diagno 
10 
Dev,ce 
jbp32 
jbp32 
10 
10 
10 
10 
Cut 
Copy 
Paste 
Delete 
Properties... 
Add Object 
Add Folder... 
Plug Device... 
Disable Device 
Download the missing device description 
Edit Object 
Edit Object With... 
Edit 10 mapping 
Import mappings from CSV... 
Export mappings to CSV... 
Diagnostics 2 
10 Link Events 2 
Messages - Total O em 
Device status 2

we can see that we were able to plug some IOL sensor from the catalog of Profinet IO-Modules, but we cannot select the IODD device added in the other page because the catalog does not include this IODD devices.

Machine generated alternative text:
Plug Device 
N ame 
@ Plug device 
Append device Insert device 
Update device 
Vend or KAII vendors:» 
String for text search 
PROFINEr 10 
SW VI. 7,27, HVV-HW 1 
Vendor 
Tur ck 
Turck 
Tur ck 
Tur ck 
Turck 
Tur ck 
Turck 
Turck 
Tur ck 
Turck 
Tur ck 
Tur ck 
Turck 
Tur ck 
Tur ck 
Version 
sw 
swv1.7.27, 
SW-SW VI. 7,27, 
SW-SW VI. 7,27, 
SW-SW VI. 7,27, 
SW-SW VI. 7,27, 
SW-SW VI. 7,27, 
SW-SW VI.7.27, HVV-HW 1 
sw 
SW-SW VI.7.27, HVV-HW 1 
SW-SW VI.7.27, HVV-HW 1 
SW-SW VI.7.27, HVV-HW 1 
SW-SW VI. 7,27, HVV-HVV 1 
SW-SW VI.7.27, HVV-HW 1 
SW-SW VI.7.27, HVV-HW 1 
SW-SW VI.7.27, HVV-HW 1 
Description 
B IN360V-QR20-10LX3-xxxx (Family) 
BINF360V-QR20-10LX3-xxxx (Family) 
B2N360-Q42 
B2N360-Q42 (Dl) 
B2N85H-QR20-10LX3-xxxx (Family) 
B2NF85H-QR20-10LX3-xxxx (Family) 
acT/NCT-Mxx-10L -xxxxx 
acT/NCT-Mxx-10L -xxxxx (Dl) 
Blx-10LU6gX2 Single Point Mode 
Blx-10LU6gX2 Point Mode 
Blx-10LU6gX2 Window Mode 
CMTH1-M12-10L6X2+1141 
CMTH1-M12-10L6X2+1141 (Dl) 
CMVT-QR20-10LX3-xxxx aso Mode 
CMVT-QR20-10LX3-xxxx aso Mode) (Dl) 
PROFINET 10 Module 
Banner Engineering 
Bosch Rexroth AG 
Buerkert Werke GmbH COKG 
Festo AG aco. KG 
Parker Hannifin 
Port configuration generic 
SIKO GmbH 
Tur ck 
BIN360V-QR20-10LX3-xxxx (Family) 
B INF360V-QR20-10LX3-xxxx (Family) 
B2N360-Q42 
B2N360-Q42 (Dl) 
B2N85H-QR20-10LX3-xxxx (Family) 
B2NF85H-QR20-10LX3-xxxx (Family) 
BCTmCT-Mxx-10L -xxxxx 
-xxxxx (Dl) 
Blx-10LU6gX2 Single Point Mode 
Blx-10LU6gX2 Two Point Mode 
Blx-10LU6gX2 Window Mode 
CMTH1-M12-10L6X2+1141 
CMTH1-M12-10L6X2+1141 (Dl) 
CMVT-QR20-10LX3-xxxx aso Mode) 
CMVT-QR20-10LX3-xxxx aso Mode) (Dl) 
Display 311 versions(for experts only) 
Group bycategory 
Display outdated versions 
Pkase sekct device fom fie 'st abowe. 
o 
(You can select another target node in the navigator while this Window is open.)